Lab 08 - Digital Logic
1 220 W resistor
2 LEDs (red and green)

To implement a simple two way light circuit using logic gates.
2 74AC00 quad 2-input NAND gate packages (supplied by UTS)
To implement a 3-variable truth table using only NAND gates.
To become familiar with digital logic gates and symbols.