Vmin
Specification
Vmax
Table LT1-3-1
Using resistors from your kit, and the provided potentiometer, design, build, test and demonstrate a circuit with the following characteristics: the output voltage, 𝑉𝑥, is adjustable from 𝑉min to 𝑉max using the potentiometer. Note that the input is a fixed DC supply, 𝑉𝑆, of value +10 V.
Ask a Lab Tutor for your specification for  𝑉min and 𝑉max .
Demonstrate the variability of Vx within the specified limits to a Lab Tutor.